IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "Project Number"
Time stamp: "2022-06-20T14:11:42"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20190108_1515(x64) - Exporter 19.2.1.1 - Alternate UI 19.2.1.1"
Application: "Autodesk Revit 2019 (ENU)" version "2019" identifier "Revit" by Organization "Autodesk Revit 2019 (ENU)"

People and organizations
  Person "Renugopal.Venkatachalam" of Organization (no name given)
  Owner history of Person "Renugopal.Venkatachalam" of Organization (no name given) | application "Autodesk Revit 2019 (ENU)" version "2019" identifier "Revit" by Organization "Autodesk Revit 2019 (ENU)" | change NOCHANGE | created 1655452588 (2022-06-17T07:56:28Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 51° 30′ 23.112487″ | longitude -0° 7′ 37.956022″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "London", "London", "United Kingdom"
      IFCBUILDINGSTOREY "Level 0" | long name "Level 0" | elevation 0.
        contains 3 elements
          1 x IFCFLOWTERMINAL | type IFCWASTETERMINALTYPE "TD3-030 Neutral channel" | object type "TD3-030 Neutral channel" | names: "ACO TD-300 Neutral channel:TD3-030 Neutral channel:308514" | material: materials ("Iron, cast", "Polymer Concrete") | property sets: IFC Parameters
          2 x IFCFLOWTERMINAL | type IFCWASTETERMINALTYPE "std(nested)" | object type "std(nested)" | names: "ZZZ_do not use_PF_ST_TaffikDrain 300 gratings_ACO:std(nested):308515", "ZZZ_do not use_PF_ST_TaffikDrain 300 gratings_ACO:std(nested):308516" | material: "Iron, cast" | property sets: IFC Parameters

Types
  IFCWASTETERMINALTYPE "TD3-030 Neutral channel" | USERDEFINED | 1 occurrence | material: materials ("Iron, cast", "Polymer Concrete") | description "ACO TD300 Neutral channel"
  IFCWASTETERMINALTYPE "std(nested)" | 2 occurrences | material: "Iron, cast" | description "ACO Grating for TraffikDrain"

Property sets
  IFC Parameters | properties | on 2 objects (2 IFCFLOWTERMINAL)
    LOD = "LOD 300" (IFCTEXT)
    Manufacturer = "ACO" (IFCTEXT)
    code_article_C_ANZRS = "142146" (IFCTEXT)
    description_C_ANZRS = "ACO TraffikDrain TD300 Transverse Grate - 0.5m" (IFCTEXT)
  IFC Parameters | properties | on 1 object (1 IFCFLOWTERMINAL)
    LOD = "LOD 300" (IFCTEXT)
    Manufacturer = "ACO" (IFCTEXT)
    code_article_C_ANZRS = "149046" (IFCTEXT)
    description_C_ANZRS = "ACO TraffikDrain TD3-030 Channel - 1m" (IFCTEXT)